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REPUBLIKA E SHQIPËRISË
MINISTRIA E MJEDISIT



Nr. _______ Prot.						               Tiranë, më ___ . 11. 2026



Request for Quotations (RFQ) - For Works

Project Title:	Clean and Resilient Environment for Blue Sea Project
Contract Ref:	AL-MTE-2.3.1/2-W-RFQ
Contract Title:	Implementation of investment plans in afforestation, pasture improvement and erosion control

Dear Contractor, 

1.	The Ministry of Environment hereby invites you to submit a quotation for the following works: 

Implementation of investment plans in afforestation, pasture improvement and erosion control, Tepelenë Municipality

2.	To assist you in the preparation of your price quotation we enclose the necessary specifications, bill of quantities and drawings, form for submitting the quotation and a draft contract form.

3.	You shall submit one original of the Price Quotation with the Form of Quotation and clearly marked “Original”.  In addition, you shall also submit one copy marked as “COPY”. Your quotation in the attached format should be sealed in an envelope and addressed to and delivered at the following address:

Ministry of Environment
Protocol Office 
Attn: Ms. Ledina Beqiraj Agalliu, Secretary General
Address: Blv. “Dëshmorët e Kombit”, No. 1, Tirana, Albania

4.	You must demonstrate relevant technical and organisational capability and sufficient financial resources to complete the Works included in this Invitation.

5.	Each bidder shall submit only one quotation, either individually, or as a partner in a joint venture. All quotations submitted in violation of this rule shall be rejected.  Partners in a joint venture shall be jointly and severally liable for the execution of the contract. In the case of a joint venture the lead partner should demonstrate work experience under paragraph 4 above.  Financial resources of all the partners in the joint venture will be combined to determine adequacy of resources. 

6.	In evaluating the quotations, the Employer will determine for each proposal the evaluated price by adjusting the price quotation by making any correction for any arithmetical errors as follows:
	(a) where there is a discrepancy between amounts in figures and in words, the amount in words will govern;
	(b) where there is a discrepancy between the unit rate and the line item total resulting from multiplying the unit rate by the quantity, the unit rate as quoted will govern;
	(c) if a Bidder refuses to accept the correction, his quotation will be rejected.

7.	Your quotation shall be valid for a period of forty five (45) days from the deadline for submission of the quotation.

8.	Your quotation in English language shall be for the whole works and based on the unit and total price indicated in the Bill of Quantities for a fixed unit rate contract. Currency of quoted prices and payment shall be Euro. The quotation shall include all duties, local taxes, customs and other levies payable by the contractor in accordance with the local laws.

9.	The Employer will award the contract to the Bidder whose quotation has been determined to be substantially responsive to this invitation to quote and who has offered the lowest evaluated price quotation and is qualified to do the work. 

10.	The contract will be governed by the terms and conditions of the attached draft Contract.

[bookmark: _Toc168299735]11.	Inspections and Audits
11.1	The Contractor shall carry out all instructions of the Project Manager which comply with the applicable laws where the Site is located.
11.2	The Contractor shall permit, and shall cause its Sub-Contractor to permit, the Bank and/or persons or auditors appointed by the Bank to inspect and/or audit its accounts and records and other documents relating to the submission of the Quotation to provide the Services and performance of the Contract. Any failure to comply with this obligation may constitute a prohibited practice subject to contract termination and/or the imposition of sanctions by the Bank (including without limitations determination of ineligibility) in accordance with prevailing Bank’s sanctions procedures.

12.	Your quotation should be submitted by November 27, 2026, 16.00 hrs. 

[bookmark: _Toc71092383]Sincerely,




Technical Specifications 
for
Implementation of Investment Plans on afforestation and erosion control,
 under the Clean and Resilient Environment for Blue Sea Project 

I. Background of the Project
The Government of Albania is implementing the Clean and Resilient Environment for Blue Sea Project (CARE4BlueSea), financed by the World Bank. The Project takes an integrated approach to preventing pollution at source in the Vjosa River Basin and along the coast. It is implemented by the Ministry of Environment through its Project Management Team.
Component 2 of the Project aims to reduce water pollution in the Vjosa River. Sub-component 2.3 reduces non-point source pollution across the basin by financing small-scale investments in nature-based solutions and sustainable land management, including improving the vegetation cover on slopes and riverbanks. Its results are measured, among others, by the indicator "Land area under sustainable landscape management practices", with a target of 200 ha.
[bookmark: _Hlk245150670]Under Sub-component 2.3, the Project Management Team engaged a technical assistance consultant to prepare a field-verified, costed and implementable investment plan for afforestation, pasture improvement and erosion control. The consultant compared candidate sites in the basin and recommended, as the pilot intervention, the forest parcels 65/a and 65/b of the Dukat–Luzat Forest Economy, in cadastral parcel no. 7 of cadastral zone 1149 (244.6 ha in all), Tepelenë Municipality. The site is included in the latest update of the State Authority for Geospatial Information as one of the two forest zones selected under Decision of the Council of Ministers No. 398, dated 13 May 2020. It burned in the 2024 fire, regenerates slowly, drains directly to the Drino and the Bënça close to their confluence with the Vjosa, is property of Tepelenë Municipality and is not used for grazing, so that no restriction of livelihoods is needed.
The site covers a planned treatment area of about 89.3 ha south of the town of Tepelenë, on the slopes between the valleys of the Bënça and the Drino, towards the village of Luzat. It lies outside the Vjosa National Park, but it drains into the Bënça and the Drino, which are part of it, so monoculture and non-native species are avoided. The approved investment plan consists of the Restoration Model and Concept Design Package and the Detailed Design, Technical Specifications and Bill of Quantities (November 2026), which prescribe aerial seeding by drone with pelleted seed of native species at 1,750 pellets per hectare. These Technical Specifications and their annexes implement that plan; the Contractor's confirmatory survey and method statement support its execution and do not replace it.
II. Objectives of the Contract
The objective of this contract is to restore forest cover on the burned and eroded slopes of the Dukat–Luzat site, so as to reduce erosion and the sediment that reaches the Drino, the Bënça and the Vjosa, and to test aerial seeding by drone, with the monitoring carried out by the Beneficiary, as a method that shortens the time of intervention on steep and inaccessible ground.
The specific objectives of the contract are:
1. Aerial seeding by drone of about 89.3 ha with certified seed of a mix of native species, in biodegradable pellets, at 1,750 pellets per hectare.
1. Protection of the soil by avoiding mechanical disturbance: no pits, terraces or machinery on the slopes.
1. Verifiable documentation of the work done may comprise treatment maps, flight records, quantities applied, simple field observations and a concise implementation record.
1. Acceptance shall follow completion of the contracted application and handover. The Contractor remains responsible for demonstrated defects attributable to its materials, coverage or workmanship for the retention period of twelve months. Germination and establishment are monitored by the Beneficiary, the forest and pasture unit of Tepelenë Municipality, outside this contract.
1. Implementation in compliance with the World Bank Environmental and Social Framework, national legislation and the protection of the Vjosa National Park downstream of the site.
The long-term outcomes (erosion control, water regime, biodiversity, landscape value) depend on establishment, protection from fire and continued management. They are not guaranteed by the Contractor beyond the correction of its own defects set in Annex 1, Section 7.
III. Scope of the Contract and Detailed Tasks
The Contractor shall carry out the services and works described below and specified in Annex 2 (Detailed Design, Technical Specifications and Bill of Quantities), under the supervision of the Supervisor appointed in writing by the Contracting Authority. The Contractor shall coordinate with the Project Management Team, Tepelenë Municipality (forest and pasture unit), the administration of the Vjosa National Park and the Civil Aviation Authority. All labour, equipment, transport, power, permits assigned to the Contractor, tests, environmental and social controls, insurance and consumables are included in the quoted prices. The quantities are given in the Priced Activity Schedule (Annex 2, Section 5).
A. Mobilisation and Readiness
1. Hold the start-up meeting with the Supervisor, Project Management Team and Municipality within the agreed mobilisation programme.
1. Submit the mobilisation package: work programme, method statement, the Contractor's Environmental and Social Management Plan, permits register, flight and emergency plans, personnel and equipment evidence, and the names of the seed sources and the pelletisation facility (deliverable D1).
1. Obtain the flight authorisation of the Civil Aviation Authority, register and ensure the aircraft, and maintain third-party liability insurance for the whole contract period.
1. Observe the conditions of the opinion of the protected areas agency, including timing restrictions and exclusion zones, and use the approved species mix.
B. Baseline Survey and Operational Mapping
1. Verify on the ground, with the forestry lead, burn effects, natural regeneration, soil depth, rock, erosion pathways, sensitive habitats and safe access in each treatment stratum.
1. The Contractor shall provide georeferenced mapping and baseline site information sufficient to define the treatment areas, exclusions, safe access and seeding plan. The Contractor may select suitable surveying methods, sensors and existing data for the site. No particular combination of sensors or fixed terrain-model accuracy is mandatory unless identified as essential in the issued scope.The net area approved by the Supervisor is the basis for measurement.
1. Clear burned debris only where a continuous layer keeps pellets from reaching the soil, and set up two take-off and landing bases.
C. Seed Supply and Pellet Production
1. The issued documents shall identify the intended native species and proportions. Seed shall come from suitable approved sources, with legally required provenance and quality documentation. Suitable alternative sources or species may be approved where availability requires. Existing seed-supplier quality information and simple visual and operational checks shall be accepted. Application quantities shall be stated in practical pellet or seed quantities, without requiring proof of viability for every individual pellet.Supply biodegradable seed pellets in an owned or directly controlled pelletisation facility, containing no pesticide, biocide, plastic or other prohibited substance; keep a material balance from seed lot to pellet batch to treated polygon.
1. The Contractor may use an environmentally acceptable biodegradable pellet formulation suitable for the approved seed and application method. No single layered construction or ingredient is mandatory. The formulation shall comply with applicable substance restrictions. The permitted use of any repellent shall be stated consistently across the issued documents.
1. Mechanical surface spreading of biodegradable seed pellets is an acceptable application method, subject to approval of its suitability for the site and species. Compatible smaller and lighter pellets, including pellets up to 10 mm in diameter, may be used. No minimum pellet mass, pneumatic implantation or fixed soil-embedding depth is required. The Contractor shall select safe flight settings and dispensing parameters suitable for the agreed coverage and application rate. Where the Contracting Authority accepts surface spreading and smaller pellets, the approved method shall not in itself be treated as a Contractor defect, and establishment results achieved with it shall not be used as evidence of a defect.
D. Calibration, Trial and Production Seeding
1. Before production seeding, the Contractor shall carry out practical dispensing and application checks appropriate to the equipment and pellets. Evidence of execution may comprise treatment maps, flight records, quantities applied and simple field observations. A separate trial block, fixed collection-tray layout, individual-pellet tracking and laboratory tests are not mandatory. The Contractor shall provide a concise implementation record using the records normally generated during the Works.Carry out the production seeding block by block, steep and high-severity zones first, at the prescribed rates, keeping daily logs and reconciling coverage with material use.
1. Suspend seeding during unsuitable wind, intense rain, saturated or frozen ground, high fire risk, wildlife disturbance or unauthorized public entry, by agreement with the Supervisor; recorded suspensions extend the dates without penalty.
The Contractor shall submit a concise completion report and the agreed application records. The Client shall accept the Works when the contracted application and handover requirements have been met and certified by the Supervisor. Routine post-seeding monitoring, repeat surveys and a mandatory twelve-month return inspection are outside this contract. Growth and survival figures are project monitoring benchmarks and are not guaranteed outcomes. The Contractor shall correct demonstrated defects attributable to its materials, coverage or workmanship for the twelve months retention period. Weather, fire, grazing, site management and other external causes shall be considered when attributing responsibility, low establishment alone is not evidence of a Contractor defect.
E. Environmental, Social, Health and Safety Requirements
1. Implement the environmental and social clauses ES-1 to ES-16 (Annex 3) and the site-specific Environmental and Social Management Plan, including labour conditions, codes of conduct, occupational health and safety, flight and community safety, pellet composition, protection of the park, waste management, chance finds and the community grievance mechanism.
1. Notify the Municipality and the residents of Tepelenë and Luzat at least three working days before the flight days, in Albanian, and keep footpaths open.
1. Not impose grazing bans, erect fences that restrict livelihoods or negotiate any access arrangement with residents; any need for an access restriction is referred to the Contracting Authority.
IV. Qualifications and Experience of the Bidder
The Bidder, or the members of a joint venture together, shall:
· Be a registered legal entity and demonstrate relevant technical and organisational capability. Evidence may include practical deployments, pilot projects, research and relevant assignments, together with the experience of the proposed team. Ongoing or completed assignments may be used. Joint ventures and named subcontractors are allowed; the Contractor remains responsible for the whole contract.
The Bidder shall present the key personnel below. Personnel shall act as the Contractor’s project team under its direction. The Contractor shall provide sufficient suitably qualified operators and technical support. Compatible functions may be combined or reassigned within the team; the personnel schedule describes functions and does not require a separate full-time person for every role. Equivalent relevant qualifications or practical expertise may be accepted, except where a particular licence is legally required. 
	
	Position
	Role in the contract
	Minimum qualification
	Minimum experience

	1.
	Project Director
	Overall supervision of the contract; accountability to the Contracting Authority; escalation; oversight of reporting, budget and stakeholder coordination
	University degree in environmental science, forestry or ecology
	5 years of project leadership, contract management or implementation

	2.
	Project Manager / Field Operations Manager
	Day-to-day implementation; operational planning; field scheduling; logistics; mobilisation of equipment; field documentation
	University degree and professional qualification in engineering, forestry, environmental management or business management
	3 years in field operations, project implementation, logistics or technical service delivery

	3.
	Forestry / Botanical / Seed Lead
	Species suitability, seed sourcing, provenance, botanical assessment, restoration methodology; signs the completion report as forest engineer
	University degree in forestry, botany, ecology, agronomy, plant or environmental science; licensed forest engineer where the law requires
	5 years in forestry, botanical or ecological work, seed sourcing, reproductive material or restoration ecology

	4.
	Drone Chief Pilot
	Plans and executes missions; safe and compliant flight operations; aircraft readiness; flight documentation
	Valid pilot licence and authorisations for the proposed operations under Albanian aviation rules
	Valid licence

	5.
	Backup Drone Pilot
	Mission continuity; operational reserve; mission set-up, loading, batteries and troubleshooting
	Valid pilot licence and authorisations for the proposed operations
	Valid licence

	6.
	Data / Spatial Analyst
	Baseline data, imagery and sensor processing, monitoring analysis, technical reporting, geographic deliverables
	University degree in remote sensing, data science, computer science, engineering or environmental informatics
	5 years in data analysis, mapping, spatial data or remote sensing

	7.
	Pelletisation Manufacturing Lead
	Production planning, pelletisation, batch control, manufacturing records and traceability
	Engineering degree, vocational qualification or equivalent practical expertise in manufacturing or process engineering
	2 years in manufacturing, coating, pelletisation, granulation or similar

	8.
	Driver / Logistics Support
	Transport of personnel, equipment, seed, pellets, batteries and consumables; field logistics
	Valid driving licence for the vehicle class
	Relevant driving or logistics experience


Curricula vitae, copies of licences where required, and the role allocation are submitted with the quotation. 
The bidder shall shall have suitable equipment lawfully available for the scheduled work::
	No
	
Equipment

	1
	1 operational seeding drone

	2
	1 spare drone for immediate replacement

	3
	Pellet dispersal mechanism with adjustable, calibratable feed control

	4
	Satellite positioning (GNSS) module for pre-planned routes

	5
	Terrain-following sensor (altitude holding at 3-4 m)

	6
	1 reconnaissance and baseline-scanning drone

	7
	Visible-light (true-colour) camera

	8
	Laser scanning sensor (LiDAR)

	9
	Thermal camera

	10
	Ground control equipment for georeferencing

	11
	Pelletisation machinery (owned or directly controlled)

	12
	Battery for the seeding drone

	13
	Chargers, generator or inverter

	14
	First Aid Kit


Equipment may be owned, rented or otherwise lawfully available to the Contractor for the scheduled work. Evidence of availability is required. The Contractor shall maintain a reasonable contingency for equipment failure; a second aircraft permanently on site is not mandatory. Operational requirements shall be met through suitable equipment and methods, without prescribing an unnecessary sensor combination or fixed flight height.V. Timeline for Completion of Tasks 
Day 0 shall be the written notice to commence following contract signature and availability of lawful site access and the necessary Clients inputs. The detailed programme and deliverable dates shall be agreed at mobilisation. Seeding shall take place as late as practical within the ecologically suitable period in 2027, after the required approvals are complete. No flight shall take place without its applicable authorisation. Delays outside the Contractor’s reasonable control, including delayed approvals despite timely complete applications, site access or unsuitable weather, shall permit an appropriate extension or the next suitable seasonal window, without delay penalties.Calendar pressure shall not override safe and ecologically suitable conditions. The Contracting Authority reviews deliverables normally within five working days; silence is not approval.
	Scope
	No.
	Deliverable
	Description
	Deadline

	Mobilisation
	D1
	Mobilisation package
	Work programme, method statement, Contractor's Environmental and Social Management Plan, permits register, equipment and staffing evidence, flight and emergency plans, occupational health and safety plan
	Within the agreed mobilisation programme and before the relevant field work.

	Baseline
	D2
	Survey and pre-seeding analysis
	Georeferenced mapping and baseline information sufficient for treatment areas, exclusions, access and the seeding plan.
	15 days after site access; before seeding

	Seeding
	D3
	Aerial Seeding
	Production seeding at the agreed application rate, using suitable equipment and a reasonable contingency. Evidence may comprise treatment maps, flight records, quantities applied and practical dispensing checks; a separate trial block and project-specific laboratory tests are not mandatory.
	Application records maintained during execution.

	Completion
	D4
	Implementation completion report 
	Concise completion report with the agreed treatment maps, flight records, quantities applied and relevant environmental and social records.
	Within the agreed close-out period after the contracted work.

	Final inspection by Supervisor
	D5
	Retention withheld Twelve months from acceptance of the completed Works. Correction of demonstrated Contractor-attributable defects, if there are.
	No routine monitoring or repeat survey. Correct proven defects attributable to the Contractor’s materials, coverage or workmanship.
	Release retention at the end of the period, subject only to a reasonable amount for notified unresolved Contractor-attributable defects.


VI. Language and Communication Requirements
Reports shall be submitted in English. 
The Contractor shall inform the Supervisor without delay of any technical, environmental, social, safety or weather issue that may affect the works or the schedule.
VII. Reporting and Coordination
The Contractor shall report to the Supervisor, who witnesses tests, certifies quantities, signs the hold points and recommends acceptance, and to the Project Management Team of CARE4BlueSea at the Ministry of Environment, which is the Contracting Authority. The Municipality is the beneficiary and manager of the forest land. The park administration may inspect the works at any time.
VIII. Period of Contract
[bookmark: _Hlk245155081]The Period of Contract shall be eight (8) months from the commencement date. The completion period shall follow the programme agreed at mobilisation and shall run from the written notice to commence. It covers the contracted mobilisation, seeding and completion report. Appropriate extensions shall apply for delays outside the Contractor’s reasonable control, including the next suitable seasonal window where needed. Acceptance shall follow completion and handover.
 
IX. Supporting Documentation 
The Bidder shall submit the following supporting documents, apart of the formal RFQ documents, with its quotation. Documents shall identify the proposed personnel, equipment and resources and demonstrate compliance with the Technical Specifications. For joint ventures and named subcontractors, the Bidder shall identify each party’s responsibilities and provide the corresponding supporting evidence.

	No.
	Requirement
	Supporting documentation to be submitted with the quotation

	A
	Bidder’s qualifications and experience
	

	A1
	Legal registration
	Copy of the business registration certificate or equivalent official document identifying the Bidder and its registered activities.

	A2
	Relevant company and project-team capability.
	Company/team profile covering relevant deployments, pilot projects, research or practical assignments

	A3
	Relevant practical assignments; ongoing or completed.
	Examples of relevant deployments, pilots, research or assignments, identifying the client or partner, scope, dates and role, with available supporting evidence. No fixed completed-contract count is required.

	A4
	Joint venture and subcontracting arrangements, where applicable
	Joint venture agreement or signed letter of intent; identification of named subcontractors; allocation of activities and resources; and signed commitments confirming their participation and availability.

	B
	Proposed personnel
	CVs or other evidence of the proposed team’s relevant qualifications or practical experience, together with a signed declaration confirming that any legally required licences are already held or will be obtained before the relevant activities commence. The Contractor shall provide the required licences before the personnel concerned undertake activities requiring them. Compatible roles may be combined or reassigned within the team.

	C
	Equipment and operational resources
	A signed declaration confirming that the Bidder either already owns or rents the necessary equipment and, if awarded the contract, will purchase, rent, lease or otherwise secure it and have it available for the relevant activities under the agreed work programme. The successful Bidder shall provide evidence of equipment availability before commencing the activities requiring that equipment.

	D
	Proposed methodology of work





SECTION 2 – DETAILED DESIGN, TECHNICAL SPECIFICATIONS AND BILL OF QUANTITIES
(ATTACHED IN A SEPARATE FILE)






































SECTION 3. FORM OF QUOTATION


									_________(Date)

		
To:_______________________________ (Employer’s Name)

     _______________________________ (Employer’s Address)

     _______________________________


We offer to execute the___________________________________________(name and number of Contract) in accordance with the Conditions of Contract accompanying this Quotation for the Contract Price of _________________________(amount in words and numbers) (______________  ) (name of currency)_____________.  We propose to complete the Works described in the Contract within a period of ______________ from the Date of Signing of the Contract. 

This Quotation and your written acceptance will constitute a binding Contract between us.  We understand that you are not bound to accept the lowest or any Quotation you receive.

We hereby confirm that this Quotation complies with the Validity of the Quotation required by the Request for Quotation.



Authorized Signature:______________________________________
Name and Title of Signatory_________________________________
			         _________________________________


Name of Contractor:_______________________________________
Address:	         _______________________________________
		         _______________________________________
Phone Number         ___________________



Fax Number, if any___________________






SECTION 4. PRICED ACTIVITY SCHEDULE


	Item
	Activity
	Unit
	Quantity
	Unit rate (EUR)
	Amount (EUR)

	1
	Preparation and Aerial Seeding (incl. Boundary marking and digital mapping; Georeferenced mapping and baseline information sufficient for the agreed seeding plan, using suitable methods selected by the Contractor.; Clearing of burned debris where it keeps pellets from the soil; Preparation of two take-off and landing bases; Flight planning and drone calibration; Drone flight and aerial seeding; Certified seed of the native species mix in biodegradable pellets, supply and delivery (156,275 pellets; 1,750 per ha); administrative expenses; technical manager (forest engineer)
	Ha
	89.3
	
	

	
	Total excl. VAT
	
	
	

	
	VAT(20%)
	
	
	

	
	TOTAL incl. VAT
	
	
	





















SECTION 5. FORM OF CONTRACT

Name of Country: Albania

Project Name: Clean and Resilient Environment for Blue Sea Project


Name of Contract: Implementation of investment plans in afforestation, pasture improvement and erosion control, Tepelenë Municipality

Contract Number: AL-MTE-2.3.1/2-W-RFQ	


This Contract is made this _______________ day of ________________2026 between Ministry of Environment on the one part (hereinafter called the Employer) and ___________ (hereinafter called the Contractor) on the other part.

Whereas the Employer has called for quotations for Contract No. AL-MTE-2.3.1/2-W-RFQ, “Implementation of investment plans in afforestation, pasture improvement and erosion control, Tepelenë Municipality”, and the Contractor has submitted a quotation for the above works and the Employer has accepted the Contractor’s Quotation dated ________  for the execution and completion of such works and the remedying of any defects therein.

Now this Contract witnesses as follows:

1. The Contractor hereby covenants to execute the works fully detailed in the Bill of Quantities included in the Contractor’s Quotation which constitute an integral part of this Contract (Annex 1) in a professional and workmanship like manner in accordance with the following Conditions of Contract:
(A) Remedy all defects within 30 days of notification by the Engineer in charge during the period of execution of the contract and thereafter defects notified within the defect liability period. The Contractor shall have 30 days to remedy it, or a reasonable longer period agreed where the nature of the work, safety, weather or seasonal conditions requires. Immediate action may be required to address an imminent safety risk.
(B) The Employer reserves the right to terminate the contract due to unsatisfactory performance 10 days after giving a written notice.  If the Contract is frustrated by the outbreak of war or by any other event entirely outside the control of either the Employer or the Contractor, the Engineer in charge shall certify that the contract has been frustrated. In such an event, both the Employer and Contractor will have a right to terminate the contract by giving 10 days notice to the other party without any financial repercussions on either side. 
(C) All material and construction equipment on site, temporary works, and Works shall be deemed to be the property of the Employer if the contract is terminated due to fault of the Contractor. The Contractor’s or any third party’s reusable operating equipment, machinery, vehicles, batteries, tools and temporary facilities shall remain their property. The Contractor shall be allowed reasonable access to remove those items safely. 
(D) The Contractor will in all cases abide by the directions of the Engineer in charge.
(a) The Contractor shall submit to the Engineer in charge, work programme, methods and schedule within the agreed mobilisation programme and before the relevant field work. 
(b) Contract completion period is eight (8) months from the commencement date. It covers mobilisation, seeding and the implementation completion report. Appropriate extensions shall apply for delays outside the Contractor’s reasonable control, including the next suitable seasonal window where needed. Acceptance shall follow completion and handover. The final inspection, by the Supervisor, takes place 12 months after the accepted seeding, at the end of the defects-liability period.
(c) In case of variations in quantities, unit rates under the contract will be used to support the variation order. New items of work performed as ordered by the Engineer in charge will be paid at the mutually agreed rate and in case of any disagreement between the Contractor and the Engineer in charge the latter will fix the unit rates that will be binding on the Contractor. 
(d) The Law governing the contract shall be applicable laws of the Government of Albania.
(e) The Contractor shall be responsible for the safety of all the activities on the Site.
(f) During execution of works the Engineer in charge will carry out inspection of works at site to verify that works are executed by the Contractor in accordance with the specifications and required quality as per specifications. Engineer in charge will reject works not performed to the required specifications and the Contractor shall take immediate actions to rectify all defects in accordance with subparagraph (a) above.
(g) Either party may terminate the Contract by giving a 30 days notice to the other for unforeseen events such as wars and acts of Gods such as earthquake, floods, fires etc. In such case the payments will be made to the date of termination of contract.
(h) The Contractor is responsible for all taxes, duties, levies, customs, etc. in accordance with the laws of the Government of Albania.
(i) The disputes between the Employer and the Contractor arising between them under or in connection the Contract shall be resolved amicably. In the event the dispute remains unresolved either party may refer the dispute to Tirana Court in accordance with the law governing the contract.

2. In consideration thereof the Employer covenants to pay the Contractor the contract price of ____________________ (in words and figures) in the following manner and installments:

(A)	Interim payments shall be due within 21 days after submission of a valid invoice for accepted work when the value of work since the previous interim payment reaches 25% of the contract amount. The final balance for accepted work shall be invoiced and paid within 21 days irrespective of that threshold, subject to the agreed retention.
	
(B)	The Employer shall retain 5% from payments for accepted work. Retention shall be released at the end of the defects-liability period without a mandatory repeat survey or return inspection. If specific Contractor-attributable defects notified during that period remain unresolved, only a reasonable amount corresponding to those defects may be withheld until they are resolved. The final payment of remaining 5 percent of the contract amount shall be made at the end of the liability period.

(C)	Final contract value will be based on the actual quantities completed.

(D)	The defect liability period will be 12 months from acceptance of completed works by the Employer.


3.	Inspections and Audits
3.1	The Contractor shall carry out all instructions of the Engineer which comply with the applicable laws where the Site is located.
3.2	The Contractor shall permit, and shall cause its Sub-Contractor to permit, the Bank and/or persons or auditors appointed by the Bank to inspect and/or audit its accounts and records and other documents relating to the submission of the Quotation to provide the Services and performance of the Contract.  Any failure to comply with this obligation may constitute a prohibited practice subject to contract termination and/or the imposition of sanctions by the Bank (including without limitation s determination of ineligibility) in accordance with prevailing Bank’s sanctions procedures.

4. Termination.
The Employer may terminate this Contract with at least ten (10) working days prior written notice to the Contractor after the occurrence of any of the events specified in paragraphs (a) through (d) of this Clause: 
(a)	If the Contractor does not remedy a failure in the performance of its obligations under the Contract within seven (7) working days after being notified, or within any further period as the Employer may have subsequently approved in writing;
(b)	If the Contractor becomes insolvent or bankrupt;
(c)	If the Contractor, in the judgment of the Employer or the Bank, has engaged in corrupt, fraudulent, collusive, coercive, or obstructive practices (as defined in the prevailing Bank’s sanctions procedures) in competing for or in performing the Contract.
(d)	If the Employer, in its sole discretion and for any reason whatsoever, decides to terminate this Contract.

In witness whereof the parties thereto have caused this Contract to be executed the day and year first before written.

	
 ________________________
 Signature (on behalf of the Employer)



	
 _________________________
 Signature on behalf of Contractor 













































SECTION 6. NOTIFICATION OF AWARD
 
Date:	                               
Procurement Reference No:		

The [name of Employer] notifies [name and address of successful Bidder] that the Quotation presented on [date] for execution of the [name and general description of Works] for the total sum of [amount in words and figures] is accepted.  A Contract Form covering this award is enclosed.
The Bidder [name] is asked to present to [name and address of Employer]:
(a) The acknowledgment copy of the Contract Form, properly signed before [date], and
(b) The acknowledgement acceptance of arithmetical errors made during evaluation [delete if no corrections were made].

.............................…….....
Employer
[name, signature and seal]



Bulevardi “Dëshmorët e Kombit” Nr.1, 1001, Tiranë  | +3554270622 | info@mjedisi.gov.al | mjedisi.gov.al
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